**Trailer/Tent Diagram**

To better support you in the set up of your stand, please illustrate on the diagram below and return with your contract.

Please label the following locations: Your Entrance, Electric Cord, Customer Window(s), Hitch, Awning (how far it opens)

\*\*We understand that some of you will be using trailers while others only tents or maybe both.

Please label the information that pertains to your site.

Length of trailer (hitch to back):\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Width of trailer: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Cords**: 120 volt must have a 3 wire male cord end / 240 volt must have a 4 wire male cord end

\*\*\*All cords must be proper amperage and be a minimum of 150 feet

|  |
| --- |
|  |

Comments or Notes: